****

**Maryville, TN**

***SCOPE***

Model: AEHD-500 Application: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Options: \_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

***OPERATING CONDITIONS***

Inlet Design Flow Rate: **500** scfm, (Std. 70°F/14.7 psia)

Inlet Design Pressure: **100** psig

Inlet Design Temperature: **100** ° F

System Design Pressure: **200** psig

Outlet Compressed Air Flow Rate:  **427** scfm (Average)

Outlet Dewpoint at Design Conditions: **-40** ° F pressure dew point

Compressed Air Purge Losses: **73** scfm (time average)

Decompression Air Losses: **0.1** scfm (time average)

NEMA Cycle Time: **8** Hrs (4 Hrs drying; 4 Hrs Regen.)

Ambient Air Temperature: **38** °F (Min.); **105**°F (Max.)

Ambient Relative Humidity: **70 %**

System Pressure Loss with Clean, Dry Filter Elements**: 5** psid

***SYSTEM COMPONENTS***

Prefilter: Coalescing filter with 0.01 μm elements

Condensate Drain: Zero-loss Electronic Drain

After Filter: Particulate filter with 1 μm elements

Final Filter: Not Applicable

Desiccant Type: Activated Alumina

Desiccant Quantity: 228 lbs./vessel

Desiccant Vessel: ASME Section VIII Division 1, “U” stamped, 200 psig at 450°F

Controller Type: Programmable Logic Controller (PLC) in NEMA 4 Enclosure

Controller Model: APC

Energy Management System: Mid-bed humidity sensor

Hygrometer (optional): Capacitive Humidity Sensor, -112°F to +68°F dew point

Switching Valves: 2 In. pneumatically operated slanted seat globe valves

Regeneration Blower: Not Applicable

Regeneration Heater: 7 KW

Regeneration Cooler: Not Applicable

Piping: 2 In. Sch. 40

Insulation: Heater shell and hot air piping protected (vessels by customer)

***DRYER ASSEMBLY***

Height: 110 inches

Width: 66 inches

Depth: 53 inches

Connection Size: 2” NPT

Dryer Assembly Weight: 2,300 pounds